<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<syntona version="0.5.18">
<module bundle="core" id="0" name="top2" type="patch">
<view height="0" width="0" xpos="20" ypos="20"/>
<modules>
<module bundle="jsyn" id="0" name="lineOut" type="lineOut">
<view height="68" width="96" xpos="558" ypos="32"/>
<jack max="1.0" min="0.0" name="input0" value="0.0" valueAdded="false"/>
<jack max="1.0" min="0.0" name="input1" value="0.0" valueAdded="false"/>
</module>
<module bundle="core" id="1" name="knob" type="knob">
<view height="60" width="68" xpos="279" ypos="26"/>
<jack max="100.0" min="0.0" name="kick" value="0.0"/>
<jack max="10000.0" min="40.0" name="in" value="592.853704"/>
<jack name="out"/>
</module>
<module bundle="core" id="2" name="knob2" type="knob">
<view height="60" width="68" xpos="279" ypos="102"/>
<jack max="100.0" min="0.0" name="kick" value="0.0"/>
<jack max="1.0" min="0.0" name="in" value="0.4024848"/>
<jack name="out"/>
</module>
<module bundle="jsyn" id="3" name="scope" type="scope">
<view height="200" width="400" xpos="368" ypos="177"/>
<jack max="1.0" min="0.0" name="input" value="0.0" valueAdded="false"/>
</module>
<module bundle="core" id="4" name="comment" type="comment">
<view height="134" width="250" xpos="11" ypos="26"/>
<text>The sawOscBL is a "band limited sawtooth wave oscillator". Note that at high frequencies there are very few aliasing artifacts. The bandlimiting is done by reducing the high energy partials used to construct the waveform.</text>
</module>
<module bundle="core" id="5" name="show" type="show">
<view height="48" width="96" xpos="398" ypos="16"/>
<jack max="1000000.0" min="-1000000.0" name="set" value="592.853704"/>
</module>
<module bundle="jsyn" id="6" name="sawOscBL" type="sawOscBL">
<view height="88" width="96" xpos="392" ypos="72"/>
<jack max="8000.0" min="40.0" name="frequency" value="592.853704" valueAdded="false"/>
<jack max="1.0" min="0.0" name="amplitude" value="0.4024848" valueAdded="false"/>
<jack name="output"/>
</module>
</modules>
<connections>
<output id="1" jack="out">
<input id="5" jack="set"/>
<input id="6" jack="frequency"/>
</output>
<output id="2" jack="out">
<input id="6" jack="amplitude"/>
</output>
<output id="6" jack="output">
<input id="0" jack="input0"/>
<input id="0" jack="input1"/>
<input id="3" jack="input"/>
</output>
</connections>
</module>
</syntona>
